Calibration Pole Strength (units of g_D)

Magnetometer Current / Pole Strength (arbitrary units)

Coil 1 Coil 2 Coil 3 Coil 4

0.95

1

1.05

1.1

1.15

1.2

1.25

1.3

10^{-1} 1 10 10^2