Electron Tagger (ET)

EET = 11:8 GeV

Photon Detector (PD)

EP D = 14:5 GeV

H1 Luminosity System IP

e p

e p

(a)

(b) (c) (d)

Figure 2: Example of a typical bremsstrahlung event detected in the H1 luminosity system: The top view of the H1 luminosity system is shown in the lower figure (a) where the location of the electron tagger (ET) and the photon detector (PD) can be seen with respect to the beam lines of e, p and the interaction point (IP). The electron tagger (b) is located directly beside the electron beampipe. A side view of the photon arm consisting of a filter (F), a water Čerenkov counter (VC) and the photon detector (PD) is shown in (c). The photon detector (d) is located in the median plane of the electron ring.